# ADDING A MARGIN

## Overview

This section explains how to move the printing position and add a margin to the left, right, or top of paper. This function is useful when characters overlap a staple or punch position.
This function can be used with the staple or punch function when a finisher of saddle finisher is installed.

Not using the Margin Shift | Using the Margin Shift
--- | ---

## Operation

### Windows

1. #### Click the [Main] tab and select "Binding Edge"

2. #### Select "Margin Shift"

   Select a target from the "Margin Shift" menu.

   ###### To change the numeric value of a margin:

   First, select a value close to the desired value from the setting items in the pull-down menu, and click the [Settings] button. Then, click or directly enter a numeric value.

### Macintosh

1. #### Select [Printer Features], then select "Binding Edge"

2. #### Select "Margin Shift"

Back to top