# CHANGING COLOUR MODE SETTING

## Overview

Change the colour mode used to scan the original.

###### Colour mode types

AUTO DETECTION | The machine detects whether the original is colour or black and white and automatically selects full colour or black and white (Mono2 or Greyscale) scanning.
Full Colour | The original is scanned in full colour. This mode is best for full colour originals such as catalogues.
Greyscale | The colours in the original are scanned in black and white as shades of grey (greyscale).
Mono2 | Colours in the original are scanned as black or white. This mode is best for text-only originals.

## Operation

1. #### Tap the [Colour Mode] key

2. #### Tap the key of the desired colour mode for the original

   If there is a mix of destinations in different send modes, tap to select a send mode (E-mail, Network Folder, FTP, or Data Entry) to set the colour mode for each mode.

3. #### If you have selected [Auto], tap the [Greyscale] key or [Mono2] key

   Specify whether Mono2 or greyscale is used when scanning black and white originals. Note that if the file format is set to JPEG, scanning will take place in greyscale.
   After the settings are completed, tap .

Back to top