# VERIFICATION STAMP CARTRIDGE

## Overview

When the verification stamp has become light, replace the verification stamp cartridge.
If a stamp unit (AR-SU1) is installed on the automatic document feeder, replace the "Verification Stamp cartridge AR-SV1 (2 pcs included)".

## Operation

1. #### Open the automatic document feeder

2. #### Remove the document backplate sheet from the automatic document feeder

   Remove the sheet slowly. Place the removed sheet with the side that was attached face up on the document glass.

3. #### Grasp the tab on the Verification Stamp unit and pull the unit out

4. #### Remove Verification Stamp cartridge (A)

5. #### Install a new Verification Stamp cartridge

6. #### Push the Verification Stamp unit back in

   Push the stamp unit in until it clicks into place.

7. #### Align the top left corner of the document backplate sheet with back left (at the tip of the mark) of the document glass

8. #### Close the automatic document feeder

   The document backplate sheet on the document glass is fixed to the automatic document feeder.

9. #### Make sure that the document backplate sheet is correctly attached to the automatic document feeder and then close the automatic document feeder

   If the document backplate sheet is not correctly attached, remove the document backplate sheet and then attach it correctly again.

Back to top