# SPLITTING A PAMPHLET BY PAGE AND TRANSMITTING THE PAGES SUCCESSIVELY (BOOK DIVIDE)

## Overview

The opened pages of a saddle-stitch pamphlet are split by page according to actual page order.
When using this function, you do not need to sort the original pages to be sent.

This function can be enabled when the original size setting is set to [Auto].
The document glass is not available for this function.

## Operation

1. #### Placing Originals into the Automatic Document Feeder

   - AUTOMATIC DOCUMENT FEEDER

2. #### Specify the destination

   - SPECIFYING A DESTINATION FROM THE ADDRESS BOOK
   - SPECIFYING A DESTINATION USING THE SEARCH NUMBER
   - ENTER A DESTINATION MANUALLY
   - SPECIFYING A DESTINATION FROM THE GLOBAL ADDRESS BOOK
   - SPECIFYING A DESTINATION FROM TRANSMISSION LOG

3. #### Tap the [Others] key, and tap the [Book Divide] key

4. #### Select the binding edge of the original

   Check the preview image displayed in the screen, and make sure that the binding edge is correct.
   After the settings are completed, tap and [Back] keys in sequence.

   ###### To cancel the book divide setting:

   Tap the [Off] key.

5. #### Tap the [Start] key to start scanning of the original

   A beep will sound to indicate that scanning and transmission have ended.
   Tap the [Preview] key to preview the output image before sending it. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
   For more information, see "CHECKING THE OUTPUT IMAGE BEFORE TRANSMISSION". However, settings for this function cannot be changed in the preview screen.

Back to top