# REMOVING CHROMATIC COLOURS FROM THE SCANNED ORIGINAL BEFORE TRANSMISSION (DROP OUT COLOUR)

## Overview

You can erase a colour area of the scanned original and send the processed original.

## Operation

1. #### Place the original

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

2. #### Specify the destination

   - SPECIFYING A DESTINATION FROM THE ADDRESS BOOK
   - SPECIFYING A DESTINATION USING THE SEARCH NUMBER
   - ENTER A DESTINATION MANUALLY
   - SPECIFYING A DESTINATION FROM THE GLOBAL ADDRESS BOOK
   - SPECIFYING A DESTINATION FROM TRANSMISSION LOG

3. #### Tap the [Others] key, and tap the [Drop Out Colour] key

   A checkmark appears on the icon.
   After the settings are completed, tap the [Back] key.

   ###### To cancel the Dropout Colour setting:

   Tap the [Drop Out Colour] key to clear the checkmark.

4. #### Tap the [Start] key to start scanning of the original

   If you inserted the original pages in the document feeder tray, all pages are scanned.
   When you place the original on the document glass, scan each page one at a time.
   After you have scanned the last original, tap the [Read-End] key.
   A beep will sound to indicate that scanning and transmission have ended.
   - Tap the [Preview] key to preview the output image before sending it. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
     For more information, see "CHECKING THE OUTPUT IMAGE BEFORE TRANSMISSION".
   - If you tap the [Function Rev.] key on the scan confirmation screen, you can change the exposure, resolution, scan size, and send size.

Back to top