# PRINTER CONDITION SETTINGS

## Default Settings

If you print data in an environment where the printer driver is not used (that is, if you print data using the MS-DOS system or if you print data using the PC that does not have the provided printer driver installed), set the detailed printing conditions. (However, the "Disable Blank Page Print" function will be effective even when the PCL printer driver is used.)

###### List of Set Up Items

Item | Setting
--- | ---
Copies | 1 to 9999 sets
Orientation | Portrait Horizontal
Default Paper Size | A3, B4, A4, B5, A5, 320 mm × 450 mm (SRA3), 225 mm × 320 mm (SRA4), 234 mm × 318 mm, 220 mm × 312 mm, 318 mm × 469 mm, 312 mm × 440 mm, 12" × 18" (A3W), 9" × 12" (A4W), 11" × 17", 8-1/2" × 14", 8-1/2" × 13-2/5" (216 mm × 340 mm), 8-1/2" × 13" (216 mm × 330 mm), 8-1/2" × 13-1/2" (216 mm × 343 mm) , 8-1/2" × 11", 7-1/4" × 10-1/2", 5-1/2" × 8-1/2", 8K, 16K
Default Output Tray | Offset Tray*1 Finisher Upper Tray Finisher Middle Tray Finisher Lower Tray Top Tray (1,2) Stacker Tray (1,2)
Default Paper Type | Plain Paper, Letter Head, Pre-Printed, Pre-Punched, Recycled, Colour
Standard Print Mode | Normal High Quality Ultra Fine
Disable Blank Page Print | (Disabled) (Enabled)
Line Thickness*1 | 0-9
2-Sided Print | 1-Sided 2-Sided (Booklet) 2-Sided (Tablet)
Colour Mode | Auto B/W
N-Up Print*2 | N-Up 1-Up 2-Up 4-Up 8-Up
Layout Left To Right*3 Right To Left*3 Upper-Left To Right*4 Upper-Left To Lower*4 Upper-Right To Left*4 Upper-Right To Lower*4
Fit To Page*5 | (Use Fit to Page) (Do not use Fit to Page)
OUTPUT | (Use Print per Unit) (Do not use Print per Unit) (Insert Before Job) Paper tray: Trays 1 to 8, bypass tray, inserter (upper/lower) (Do not Insert Before Job) (Insert After Job) Paper tray: Trays 1 to 8, bypass tray, inserter (upper/lower) (Do not Insert After Job) Staple Position: None, 1 Staple at Back, 2 Staples, 2 Staples (Top) (Slant Staple)*1 (Do not Slant Staple)*1 (Use Punch) (Do not use Punch) Punch Position 2holes, 3holes, 4holes
Fold | Enabled Disabled
Saddle Fold Z-Fold C-Fold Accordion Fold Double Fold Half Fold
Trimming Width Settings | 2.0 to 20.0 mm
QUICK FILE | (Save data in Quick File mode) (Do not save data in Quick File mode)

*1 This setting is used to adjust the line width of vector graphics. Except for CAD and other specialized uses, there is normally no need to change this setting. When "0" is selected, all lines are printed at a width of 1 dot.
*2 Paper sizes that can be used with this function are A3, B4, A4, 11" × 17", 8-1/2" × 14", 8-1/2" × 11",11" × 17", 8-1/2" × 14" and 8-1/2" × 11". (This function may not take effect with some print methods.)
*3 Can be selected when 2-Up is selected.
*4 Can be selected when 4-Up/8-Up is selected.
*5 Only effective when printing PDF, JPEG, and TIFF files.

- When printing using the printer driver, the printer driver settings take precedence over the printer condition settings.
- The display varies depending on the peripheral devices installed.

## PCL Settings

This is used to set the symbol sets, fonts, and line feed code used in a PCL environment.

###### List of Set Up Items

Item | Description | Setting
--- | --- | ---
PCL Symbol Set Setting | Specify the symbol set used for printing. | Select from 35 items
PCL Font Setting | Select a font used for printing. | Internal Font Extended Font (List of internal fonts when extended fonts are not installed)
PCL Line Feed Code | This setting is used to select how the printer responds when a line feed command is received. | 0.CR=CR; LF=LF; FF=FF 1.CR=CR+LF; LF=LF;FF=FF 2.CR=CR; LF=CR+LF; FF=CR+FF 3.CR=CR+LF; LF=CR+LF; FF=CR+FF
Wide A4 | When this is enabled, 80 characters per line are printed on the A4 (8-1/2" × 11") size paper using a 10-pitch font. (When this setting is disabled, up to 78 characters are printed per line.) | (Enabled) (Disabled)

## PostScript Settings

When an error occurs during PostScript printing, these settings determine whether or not an error notice is printed and whether or not the PostScript data is received in binary format.

###### List of Set Up Items

Item | Description | Setting
--- | --- | ---
Screen Setting | Select print quality settings. | Normal Text/Photo Text Photo Dot (High Line Number) Dot (Low Line Number)
Print PS Error | When a PS (PostScript) error occurs during PostScript printing, this setting determines whether or not an error notice is printed. | (Enabled) (Disabled)
Binary Processing | Receive PostScript data in binary format. | (Enabled) (Disabled)
Store Print Data in PS Format | Save the print data in PS format. | (Enabled) (Disabled)

Back to top