# SETTING FOR PRINT FROM THE MFP (SMB)

## Setting for Print from the MFP(SMB)

Allows you to access the network folder from the machine operator panel, and to select network folder data for printing.

### Adding or editing a Network Folder

When the [Add] key is tapped, the network folder registration screen appears. Up to 20 network folders can be registered.
When you tap a network folder name, the registration screen for that network folder appears. You can now edit it.

###### List of Set Up Items

Item | Description
--- | ---
Name | Enter a name to be displayed on the machine operator panel.
Folder Path | Enter a path to the network folder.
Enable User Authentication | Enables user authentication. The user name and password are required to enter.
User Name | Enter the user name used for logging in the network folder.
Password | Enter the password required for logging in the network folder. To change the password, set [Change Password] to and enter the new password in the text box.

### Deleting a Network Folder

To delete a selected network folder, set the checkbox at the left of the network folder name to and tap [Delete] key.
Back to top