# PERIPHERAL DEVICES

## Overview

Peripheral devices can be installed on the machine to increase its range of functionality.
Peripheral devices are generally optional. However, some models include certain peripheral devices as standard equipment.

(As of March 2013)

Product name | Product number | Description
--- | --- | ---
Large capacity tray | MX-LC12 | Additional tray. A maximum of 3,500 sheets of paper can be placed.
MX-LCX3 N | Additional tray. A maximum of 3,000 sheets of paper can be placed.
Large capacity trays | MX-LC13 | Additional tray. A maximum of 5,000 sheets of paper can be placed.
Multi bypass tray | MX-MF10 | Additional tray. A maximum of 500 sheets of paper can be placed. Install this tray in the machine.
MX-MF11 | Additional tray. A maximum of 500 sheets of paper can be placed. Install this tray on the large capacity trays.
Long paper feeding tray | MX-LT10 | When using long paper, the long paper is loaded in the bypass tray.
Exit tray unit | MX-TR14 | Output tray to be installed in the right of the machine.
Paper pass unit | MX-RB14 | This unit is required for installing large capacity trays.
Connection module | MX-RB17 | This unit is required to facilitate connection of two large capacity trays.
Exit tray cabinet | MX-TU14 | Output tray to be installed in the centre of the machine. This unit is required when a finisher or saddle finisher is not installed.
Finisher | MX-FN21 | Output device that enables the use of the staple function and offset function. A maximum of 100 sheets of paper can be stapled.
Saddle stitch finisher | MX-FN22 | Output device that enables use of the staple function, offset function and pamphlet copy function. A maximum of 100 sheets of paper can be stapled.
High capacity stacker | MX-ST10 | This unit is useful when you output a large number of copies. A maximum of 5,000 sheets of paper can be output.
Paper cart | MX-CA10 | This is a cart that is installed in the high capacity stacker. It is useful when you carry a large number of output sheets. One unit of this product is supplied with MX-ST10, and this is for addition.
Punch module (100-sheet punching) | MX-PN13A, MX-PN13B, MX-PN13C, MX-PN13D | This unit punches holes in copies and other output. A finisher or saddle finisher is required.
Trimming module | MX-TM10 | This unit trims the excess portions of saddle-stitched sheets. A saddle finisher (100-sheet stapling) is required.
Folding unit | MX-FD10 | This unit folds and outputs paper. A finisher (100-sheet stapling) or saddle finisher (100-sheet stapling) is required.
Inserter | MX-CF11 | This unit inserts covers and insertion sheets. This unit can also feed paper to a finisher (100-sheet stapling) or saddle finisher (100-sheet stapling) for finishing.
Curl correction unit | MX-RB15 | This unit corrects curls in printed paper. This unit is required for installing a finisher (100-sheet stapling), saddle finisher (100-sheet stapling), folding unit, or inserter.
Paper pass unit | MX-RB12 | This unit is required for installing a finisher or saddle finisher.
MX-RB13 | This unit is required for directly installing a finisher (100-sheet stapling) or saddle finisher (100-sheet stapling) and inserter.
Barcode Font Kit | MX-PF10 | Adds barcode fonts to the machine.
XPS expansion kit | MX-PUX1 | This kit can be used as an XPS compatible printer. Please consult your dealer for details.
Mirroring kit | MX-EB15 | Stores a copy of data in a separate place.
Application Integration Module | MX-AMX1 | The application integration module can be combined with the network scanner function to append a metadata file to a scanned image file.
Enhanced compression kit | MX-EB11 | Saves a scanned document in the High Compression PDF format. High Compression PDF results in a smaller size than regular PDF.
Application Communication Module | MX-AMX2 | This links the machine to an external application over a network.
Keyboard | MX-KB13 | This is a keyboard that is integrated with the machine. When not in use, it can be stored under the operation panel.
Web browsing expansion kit | MX-AM10 | Internet access is enabled for viewing Web pages.
Stamp unit | AR-SU1 | This stamps each original page after it is scanned in image send mode. An automatic document feeder is required.
Stamp cartridge | AR-SV1 | Two Verification Stamp cartridges are included.
Staple cartridge | MX-SCX2 | Staples paper. A finisher or saddle finisher is required.
MX-SCX1 | Saddle stitches paper. A saddle finisher is required.
Status indicator | MX-SL10 N | The status of the machine is indicated.

Some options may not be available in some countries and regions.
Back to top