# INTERIOR

This section describes the names and functions of the respective parts inside the machine.
Tap the name to make its details pop up.

×
Toner cartridge
This cartridge contains toner. When the toner in a cartridge runs out, the cartridge of the colour that ran out must be replaced.
-TONER CARTRIDGE
×
Fusing unit
Heat is applied here to fuse the transferred image onto the paper.
The fusing unit is hot. Exercise care not to burn yourself when removing a misfeed.
×
Transfer belt
This belt takes the image formed with toner off the photoconductive unit and transfers the image onto paper.
Do not touch or damage the transfer belt.
This may cause a defective image.
×
Right side cover
Open this cover to remove a misfeed.
×
Paper reversing section cover
This unit is used for reversing paper when 2-sided printing is performed. Open this cover to remove a paper misfeed.
×
Main power switch
Use this switch to turn on the machine's power.
-TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE
×
Waste toner box
This box collects excess toner that is produced during printing.
-WASTE TONER BOX
A service technician collects replaced waste toner boxs.
×
Right side cover release lever
To remove a paper misfeed, pull and hold this lever up to open the right side cover.
Back to top