# NETWORK STATUS

The Network Status screen shows the general status information and the statuses relevant to, TCP/IP, NetWare, EtherTalk, and NetBIOS protocols.

Item | Description
--- | ---
General | Displays the information common to the network. Link Status: Displays the data transfer rate of the NIC and cable information. Duplex Mode: Displays the duplex mode of the NIC. Hardware Address: Displays the MAC address of the NIC. Print Status on Startup: Displays whether or not status is printed upon startup. Device Name: Displays the device name. Domain Name: Displays the domain name.
TCP/IP | Displays the current status of the TCP/IP protocol. IPv4 Settings: Displays the IPv4 protocol settings. DHCP/BOOTP: Selects whether or not the IP address is obtained from the DHCP/BOOTP server. RARP: Displays the status of the RARP protocol. IPv4 Address: Displays the IPv4 address. Subnet Mask: Displays the current subnet mask. Default Gateway: Displays the current default gateway. IPv6 Settings: Displays the IPv6 status. DHCPv6: Displays the status of the DHCPv6 server. Manual Address: Displays the IPv6 address that has been manually specified. Default Gateway: Displays the current default gateway. Link-Local Address: Displays the link-local address. Stateless Address 1: Displays the stateless address. Stateless Address 2: Displays the stateless address. Stateful Address: Displays the stateful address.
DNS | Displays the status of the DNS server. Primary Server: Displays the current IP address of the primary DNS server. Secondary Server: Displays the current IP address of the secondary DNS server. Domain Name: Displays the current domain name of the DNS server.
WINS | Displays the status of the WINS server. Primary Server: Displays the current IP address of the primary WINS server. Secondary Server: Displays the current IP address of the secondary WINS server. Primary Server (DHCP): Displays the current IP address of the primary WINS server (DHCP). Secondary Server (DHCP): Displays the current IP address of the secondary WINS server (DHCP). Scope ID: Displays the current WINS scope ID. Scope ID (DHCP): Displays the current WINS scope ID (DHCP).
NetWare Status | Displays the NetWare status. NetWare: Displays the status of the NetWare protocol. Frame Type: Displays the frame type. Network Number: Displays the network number. Operation Mode: Displays the operation mode. PSERVER Name: Displays the print server name. NDS Tree: Displays the NDS tree name. NDS Context: Displays the NDS context.
EtherTalk Status | Displays the EtherTalk status. EtherTalk: Displays the status of the EtherTalk protocol. Zone Name: Displays the zone name. Type Name: Displays the type name. Object Name: Displays the object name.
NetBIOS Status | Displays the NetBIOS status. NBT/WINS: Displays NBT/WINS protocol status. Master Browser: Displays the Master Browser.

Back to top