# ADJUSTING RED / GREEN / BLUE IN COPIES(RGB)

## Overview

This function selects any one of the three colour components R (red), G (green), and B (blue) to increase or decrease the selected colour tone.

RGB must be specified before scanning the original.

## Operation

1. #### Tap the [Others] key, and tap the [RGB Adjust] key

2. #### Tap the key of the colour you want to adjust

3. #### Tap or slide the slider to adjust the colour

   After the settings are completed, tap and the [Back] key in sequence.

   Only one colour can be adjusted. If you adjust one colour and then adjust another colour, the adjustment of the first colour is cancelled.

   ###### To cancel the RGB Adjust setting:

   Tap the [Off] key.

4. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

5. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

6. #### Tap the [Colour Start] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

Back to top