# SPECIFYING A DESTINATION FROM TRANSMISSION LOG

## Overview

Select a destination from the transmission log.
The most recent 50 addresses are displayed for destinations of Image Send.

- When a destination for retransmission is selected in the transmission log screen, the mode of the selected destination is automatically selected.
- The following types of addresses are not stored for resending.
  - One-touch key for a contact or group in which multiple destinations are stored
  - Broadcasted addresses
  - Destinations transmitted to using a program
- The user names and passwords for destinations other than those stored in the network folder are not stored for security reasons. If a screen requiring you to enter such information appears, enter the information again.
- The addresses shown in the transmission log can be stored in an address book. However, addresses of the FTP transmission cannot be stored from the machine.

## Operation

1. #### Tap the [Select among addresses recently sent to] key on the action panel

2. #### Tap the destination key

   If a screen requiring you to enter the user name and password appears, enter the information.

   When you select the destination and tap the [New Registration with Address Book] or [Additional Registration with Address Book] key, the destination can be stored in the address book.

   ###### To cancel the resend setting:

   Tap the [Clear] key to release the selection.

Back to top