# ENTER A DESTINATION MANUALLY

## Overview

In Scan to E-mail mode, you can directly enter a destination to specify it. In Scan to Network Folder mode, you can directly specify a reference.
For Scan to FTP, you cannot manually enter a destination.

## Operation

1. #### Tap Address text box

   - In data entry mode, select the mode of the destination, and enter the destination address.
   - If you tap Address text box in Scan to FTP, the address book screen appears.

2. #### Use the soft keyboard to enter a destination address

   - For Scan to Network Folder mode, the network folder entry screen appears. See "Specifying a network folder as an address".
   - After entering the destination address, tap the [OK] key.
   To switch among [To], [Cc] and [Bcc], tap .
   You can select [Bcc] if [System Settings] → [Image Send Settings] → [Scan Settings] → [Scan Settings] → [Bcc Setting] are selected and if [Enable Bcc] is enabled.

### Specifying a network folder as an address

1. #### Tap the [Browse] key

   - To directly enter a destination, tap the [Path Input to Folder] key. The soft keyboard is displayed.
   - If a user name and password are required, check with your server administrator and enter them.

2. #### Tap the key of the workgroup that you wish to access

   - Tap and enter a keyword to search for a workgroup, server, or network folder.
   - Up to 100 workgroups, 100 servers, and 100 network folders are displayed.
   - Tap to return to the screen of step 1.

3. #### Tap the key of the server or computer that you wish to access

   If a screen appears prompting you to enter a user name and password, check with your server administrator and enter the appropriate user name and password.

4. #### Tap the key of the network folder

   After the settings are completed, tap the [Enter] key. You will return to the screen of step 1. Tap the [Enter] key again to accept the destination.

Back to top