# SCANNING THIN ORIGINALS (SLOW SCAN MODE)

## Overview

Use this function when you wish to scan thin originals using the automatic document feeder. It helps prevent thin originals from misfeeding.

When slow scan mode is selected, 2-sided scanning is not possible.

## Operation

1. #### Placing Originals into the Automatic Document Feeder

   Adjust the original guides slowly.
   - AUTOMATIC DOCUMENT FEEDER

   If the originals are inserted using excessive force, they may crumple and misfeed.

2. #### Specify the destination

   - SPECIFYING A DESTINATION FROM THE ADDRESS BOOK
   - SPECIFYING A DESTINATION USING THE SEARCH NUMBER
   - ENTER A DESTINATION MANUALLY
   - SPECIFYING A DESTINATION FROM THE GLOBAL ADDRESS BOOK
   - SPECIFYING A DESTINATION FROM TRANSMISSION LOG

3. #### Tap the [Others] key, and tap the [Slow Scan Mode] key

   A checkmark appears on the icon.
   After the settings are completed, tap the [Back] key.

   ###### To cancel the slow scan mode setting:

   Tap the [Slow Scan Mode] key to clear the checkmark.

4. #### Tap the [Start] key to start scanning of the original

   A beep will sound to indicate that scanning and transmission have ended.
   Tap the [Preview] key to preview the output image before sending data. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
   For more information, see "CHECKING THE OUTPUT IMAGE BEFORE TRANSMISSION". However, settings for this function cannot be changed in the preview screen.

Back to top