# NETWORK SETTINGS LIST

## Overview

The following is a list of setting mode items, factory default settings and restrictions for each item.
Depending on the machine specifications and peripheral devices installed, it may not be possible to use some settings.
U: General user; A: System administrator / Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Network Settings
| Quick Settings
| No | Yes
| IPv4 Settings
| - | No | Yes
| IPv6 Settings
| - | No | Yes
| Network Name Settings
| - | No | Yes
| DNS Settings
| - | No | Yes
| SMTP Settings
| - | No | Yes
| LDAP Settings
| - | No | Yes
| Public Folder / NAS Setting
| - | No | Yes
| General Settings
| No | Yes
| General Settings
| No | Yes
| Print Status on Startup
| Disable | No | Yes
| Network Settings
| - | No | Yes
| Reset the NIC
| - | No | Yes
| PROTOCOL SETTINGS
| No | Yes
| TCP/IP
| No | Yes
| TCP/IP Settings
| No | Yes
| TCP/IP
| Enable | No | Yes
| IPv4 Settings
| No | Yes
| DHCP/BOOTP
| Disable | No | Yes
| RARP
| Disable | No | Yes
| IPv6 Settings
| No | Yes
| IPv6
| Disable | No | Yes
| DHCPv6
| Enable | No | Yes
| Ping Command
| No | Yes
| NetWare
| No | Yes
| NetWare Settings
| No | Yes
| NetWare
| Disable | No | Yes
| Frame Type
| 802.2 | No | Yes
| Operation Mode
| PSERVER | No | Yes
| PSERVER Settings
| No | Yes
| Bindery Mode
| Enable | No | Yes
| RPRINTER Settings
| - | No | Yes
| EtherTalk
| No | Yes
| EtherTalk Settings
| No | Yes
| EtherTalk
| Disable | No | Yes
| NetBIOS
| No | Yes
| NetBIOS Settings
| No | Yes
| NBT/WINS
| Disable | No | Yes
| SERVICE SETTINGS
| No | Yes
| DNS
| - | No | Yes
| WINS
| - | No | Yes
| SMTP
| - | No | Yes
| SNMP
| - | No | Yes
| Kerberos
| - | No | Yes
| SNTP
| - | No | Yes
| mDNS
| - | No | Yes
| PRINT PORT SETTINGS
| No | Yes
| LPD
| No | Yes
| LPD Settings
| No | Yes
| LPD
| Enable | No | Yes
| Timeout
| 0 seconds | No | Yes
| Use Banner
| Disable | No | Yes
| RAW
| No | Yes
| Raw Print Settings
| No | Yes
| Raw Print
| Enable | No | Yes
| Port Number
| 9100 | No | Yes
| Timeout
| 90 seconds | No | Yes
| Use Bidirectional
| Disable | No | Yes
| WSD
| No | Yes
| WSD Settings
| No | Yes
| WSD Print
| Enable | No | Yes
| Use Multicast Discovery
| Enable | No | Yes
| LDAP Settings
| No | Yes
| LDAP Settings
| Enable | No | Yes
| Global Address Books List
| - | No | Yes
| Public Folder / NAS Setting
| No | Yes
| Public
| Use of Storage
| Allowed | No | Yes
| Shared
| Use of Storage
| Allowed | No | Yes
| Proxy Setting
| No | Yes
| Proxy Server Address
| - | No | Yes
| User Name
| - | No | Yes
| Password
| - | No | Yes
| Port Number
| 8080 | No | Yes
| Address without Using Proxy
| - | No | Yes
| HTTP Access Settings
| No | Yes
| Number of Users who can Log-in at the Same Time
| 32 | No | Yes
| Auto Logout Time
| 60 | No | Yes
| View Login User
| - | No | Yes

Back to top