# COPYING BOTH SIDES OF A CARD AS A SINGLE PAGE (CARD SHOT)

## Overview

This function copies the front and reverse sides of a card on one sheet.
This function is convenient for making copies for identification purposes.

###### To change the default original size during Card Shot:

In "Setting mode (administrator)", select [System Settings] → [Copy Function Settings] (Tab) → [Copy Function Settings] → [Card Shot Settings].

## Operation

1. #### Select the paper to be used for card shot

   - SETTING THE PAPER TRAY
   - SETTING THE BYPASS TRAY

2. #### Tap the [Others] key, and tap the [Card Shot] key

3. #### Tap the [On] key, and specify the original size

   After the settings are completed, tap and the [Back] key in sequence.

   - Tap the areas displaying width and height sizes of the original respectively, and enter the sizes using the numeric keys.
     Or tap to enter the width and height sizes.
   - When you set the [Adjust to Paper Size] checkbox to , the original is enlarged or reduced by the ratio appropriate to the original size.

   ###### To cancel the Card Shot settings:

   Tap the [Off] key.

4. #### Place a card face down on the document glass, and tap the [Preview] key

   - DOCUMENT GLASS

5. #### Place a card face up on the document glass, and tap the [Additionally Scan] key to scan the reverse side

   Copy settings cannot be changed when scanning additional pages.

6. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

7. #### Tap the [Read-End] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

Back to top