# SERVICE SETTINGS

## "DNS" Tab

Use this tab to configure DNS settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### DNS Settings

###### Primary Server

Enter the IP address of primary DNS server.

###### Secondary Server

Enter the IP address of secondary DNS server.

###### Timeout

Enter a timeout. The default setting is 20 seconds.
This time is used until the connection to the DNS server is established according to the standard specifications.

###### Domain Name

Enter the domain name where the selected DNS server exists.

###### Dynamic DNS Updating

Set this option to use the dynamic updating of DNS server.

###### Updating Interval

Enter an interval to update the DNS server.

## "WINS" Tab

Use this tab to configure WINS settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### WINS Settings

###### Primary Server

Enter the IP address of primary WINS server.

###### Secondary Server

Enter the IP address of secondary WINS server.

###### Scope ID

Enter the scope ID.

## "SMTP" Tab

Use this tab to configure SMTP settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### SMTP Settings

###### Primary Server

Enter the IP address or the host name of the primary SMTP server.

###### Secondary Server

Enter the IP address or the host name of the secondary SMTP server.

###### Port Number

Enter a port number. The default setting is port 25.

###### Timeout

Enter a timeout. The default setting is 20 seconds. This value is used for connection to the SMTP server and for data transmission according to the e-mail system specifications.

###### Reply E-mail Address

If data transmission has failed, the undelivered e-mail may be returned from the server.
Enter an e-mail address (a single address only) to receive such undelivered mails.
Usually, enter the e-mail address of the system administrator.

###### Enable SSL

If is selected, the SMTP-over-TLS encryption communication can be used by STARTTLS command.
This requires the server to support the STARTTLS command.
To allow SSL communication, set the "Port Number" to the same port number as the normal SMTP.

###### SMTP Authentication

If is set, the SMTP server authentication is carried out.
If you use the Kerberos authentication, set the KDC server, port number, and realm on the Kerberos authentication settings page.

###### User Name

Enter the user name.

###### Password

Enter the password.
To change the password, set [Change Password] to .

###### POP before SMTP

If is set, you are authenticated to the POP server before using the SMTP communication.

- POP3 Server: Enter the IP address or the host name of the secondary SMTP server.
- Port Number: Enter the POP3 port number for POP before SMTP communication. The default setting is port 110.
- POP Authentication: If is set, the authentication protocol (including APOP) is used for authentication to the POP3 server.
- User Name: Enter the user name for POP before SMTP communication.
- Password: Enter the password required for POP before SMTP communication. To change the password, set [Change Password] to .
- Enable SSL: If set to , the POP over SSL communication or the POP over TLS communication by STLS command is enabled.
  This requires the server to support the POP over SSL communication or the STLS command.
  To allow SSL communication, set the "Port Number" to the POP over SSL communication port number.
  To allow POP over TLS communication, set the "Port Number" to the same port number as for the normal POP3 communication.

###### Connection Test

Tap the [Execute] key to test the connection to the SMTP server.

## "SNMP" Tab

Use this tab to configure SNMP settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### SNMP v1 Settings

Set this option to use the SNMPv1 settings.

###### Access Method

Set an access method.

###### GET Community

Enter the GET community name to fetch the device information using SNMP.

###### SET Community

Enter the SET community name required for SNMP setting.
To change the SET community, set .

###### TRAP Community

Enter the community name to be used for the SNMP TRAP sent from the device.

###### TRAP Target Address

Enter the IP address of the destination computer for SNMP TRAP communication.

### SNMP v3 Settings

Set this option to use the SNMPv3 settings.

###### User Name

Enter the user name.

###### Authentication Key

Enter the authentication key.

###### Privacy Key

Enter the privacy key.

###### Context Name

The context name is displayed.

## "Kerberos" Tab

Use this tab to configure Kerberos settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### Kerberos Authentication Settings

###### KDC Server

Enter the IP address or host name of the Kerberos authentication server.

###### Port Number

Enter the port number of the Kerberos authentication server. The default setting is port 88.

###### Realm

Enter the Kerberos realm.

## "SNTP" Tab

Use this tab to configure SNTP settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### SNTP Settings

###### SNTP

Set this option to use the SNTP protocol.

###### SNTP Server

Enter the IP address or host name of the SNTP server.

###### Port Number

Enter a port number. The default setting is port 123.

###### Timeout

Enter a timeout. The default setting is 5 seconds.

###### Synchronous Interval

Enter an interval to synchronize to the SNTP server.

###### Synchronize Upon Start

To establish synchronization during machine startup, set to .

###### Synchronize Now

When tapped, the machine is synchronized with the SNTP server time.

## "mDNS" Tab

Use this tab to configure mDNS settings.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### mDNS Settings

###### mDNS

Set this option to use the mDNS settings.

###### Service Name

Enter a service name.

###### Domain Name

Enter the domain name.

###### Priority Service

Select a service you use with the priority.
Back to top