# COPYING SEQUENCE

Change from the Home Screen or each mode to copy mode, and follow the steps below.

- SELECTING COPY MODE

- Maximum print area: 319 mm x 480 mm
- Image quality assurance range: 303 mm

## Operation

1. #### Place the original

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

2. #### Scan the original

   Tap the [Preview] key to scan the original.

   - To scan a 2-sided original, configure the 2-sided copy settings before scanning the original.
   - When not checking the preview image, tap the [Colour Start] or [B/W Start] key to start copying.

3. #### Check the preview image

   Check the settings such as the colour, 2-sided state, and staple position on the Preview screen.

4. #### Start copying

   Tap the [Colour Start] or [B/W Start] key.
   - To make two or more copies, tap the copies display key to set a number of copies.

   - To cancel the number of copies, tap the [C] key (in the numeric keys).
   - To cancel a copy job, tap the [Cancel Print] key.
   - If you tap the [File] key or [Quick File] key on the action panel before starting copying, you can save the scanned original as data.
   - - SAVING DATA IN QUICK FILE MODE
     - SAVING SCANNED ORIGINAL DATA

Back to top