# CLEANING THE MACHINE

To ensure that the machine continues to provide top quality performance, periodically clean the machine.
If coloured/white lines or misfeeds occur, clean the following parts.

When dirty spots or coloured/white lines are left on scanned images: | DOCUMENT GLASS DOCUMENT BACKPLATE SHEET SCANNING AREA
When paper misfeed occurs in the bypass tray: | BYPASS FEED ROLLER
When coloured lines appear: | LASER UNIT

Do not use a flammable spray to clean the machine. If gas from the spray comes in contact with hot electrical components or the fusing unit inside the machine, fire or electrical shock may result.

- Do not use thinner, benzene, or similar volatile cleaning agents to clean the machine. These may degrade or discolour the housing.
- Use a soft cloth to gently wipe off dirt from the operation panel. If you use a stiff cloth or rub hard, the surface may be damaged.

Back to top