# MAKING A COPY ON TABS OF TAB PAPER (TAB COPY)

## Overview

This function makes a copy on tabs of tab paper.
Prepare appropriate originals for tab captions.

### The positions to place the originals and tab paper

The following shows how to load tab paper for right binding or left binding.

###### Tab for left binding

Originals | SETTING ORIGINALS | Loading tab paper
--- | --- | ---

###### Tab for right binding

Originals | SETTING ORIGINALS | Loading tab paper
--- | --- | ---

Tab Copy must be specified before scanning the original.

###### To change the default image shift width for tab copying:

In "Setting mode (administrator)", select [System Settings] → [Copy Function Settings] (Tab) → [Copy Function Settings] → [Initial Tab Copy Setting].
The default image shift width can be set from 0 mm to 20 mm (0" to 5/8"). The factory default setting is 10 mm (1/2").

## Operation

1. #### Tap the [Others] key, and tap the [Tab Copy] key

2. #### Tap the [On] key

3. #### Sets an image shift width (tab width)

   Tap the numeric value display field, and enter the image shift width using the numeric keys.
   Or tap to enter the image shift width.
   After the settings are completed, tap and the [Back] key in sequence.

   ###### To cancel the tab copy setting:

   Tap the [Off] key.

4. #### Load the tab paper

   The width of the tab paper can be as wide as A4 width (210 mm) plus 20 mm (or 8-1/2" × 11" paper (8-1/2") plus 5/8").

5. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

6. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

7. #### Tap the [Colour Start] or [B/W Start] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

Back to top