# ADJUSTING RESOLUTION WHEN SCANNING (SCAN RESOLUTION)

## Overview

This function adjusts the resolution when scanning the original, enabling the high-quality output or speed-priority output according to the application.

- Scan Resolution must be specified before scanning the original.
- The scan resolution setting is applied when making a full-size black & white copy.

## Operation

1. #### Tap the [Others] key, and tap the [Scan Resolution] key

2. #### Select the resolution

   The resolution can be set to both the document feeder and document glass.
   After the settings are completed, tap and the [Back] key in sequence.

3. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

4. #### Tap the [B/W Start] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

Back to top