# RESENDING TO UNSUCCESSFUL BROADCAST TRANSMISSION DESTINATIONS

The results of a completed broadcast transmission can be checked in the job management screen. If transmission to any destination has failed, you can send to the same destination again.

## Operation

1. #### Tap the Job Management display, and tap the [Scan] tab

2. #### Tap the [Complete] key

3. #### After tapping the key of the completed broadcast transmission, tap the [Check Details of Selected Job] key on the action panel

   The details of the job appear.

   - "Broadcast xxxx" will appear as the address of the broadcast job key. The job control number that appeared on the touch panel when scanning ended appears in "xxxx".
   - If the broadcast transmission included destinations of different modes, the same broadcast transmission key will appear in each of those modes.

4. #### After tapping the [Failed] tab, tap the [Resend to All Addresses Which Failed in Sending] key on the action panel

   The machine starts resending the image to the unsuccessful broadcast transmission destinations.

   The steps to follow after the [Resend to All Addresses Which Failed in Sending] key is tapped differ depending on whether or not the Document Filing function is used.

   - ###### Using document filing:

     When you enter the unsuccessful destination, you will return to the document filing resend screen.
     Perform the document filing resend procedure. (There is no need to re-scan the original.)

   - ###### When document filing is not used:

     When you enter the unsuccessful destination, you will return to the initial screen. Place the original and perform the steps of the broadcast transmission.

Back to top