# ADJUSTING THE INTENSITY (SATURATION) OF A COPY (INTENSITY)

## Overview

This function adjusts the intensity (saturation) of a colour copy image.

[Intensity] must be specified before scanning the original.
This function cannot be combined with [Copy of Copy] or [Colour Tone Enhancement] in Exposure.

## Operation

1. #### Tap the [Others] key, and tap the [Intensity] key

2. #### Tap or slide the slider to adjust the intensity

   After the settings are completed, tap and the [Back] key in sequence.

   ###### To cancel the intensity setting:

   Tap the [Off] key.

3. #### Place an original, and tap the [Preview] key

   Place the original in the automatic document feeder or on the document glass.
   - AUTOMATIC DOCUMENT FEEDER
   - DOCUMENT GLASS

4. #### Check the preview image in the preview screen

   ###### To cancel all settings:

   Tap the [CA] key.

5. #### Tap the [Colour Start] key to start copying

   ###### To make two or more sets of copies:

   Tap the copies display key to specify the number of copies.

Back to top