# SETTING FOR PRINT FROM THE MFP (FTP)

From the operator panel of machine, you can access the FTP server and select server data for printing.

### Adding or editing an FTP server

When the [Add] key is tapped, the FTP server registration screen appears. Up to 20 network folders can be registered.
When you tap an FTP server name, the registration screen for that FTP server appears. You can now edit it.

###### List of Set Up Items

Item | Description
--- | ---
Name | Enter a name to be displayed on the machine operator panel.
FTP Server | Enter the IP address or host name of the FTP server.
Directory | Enter the destination directory of the FTP file server.
Enable User Authentication | Enables user authentication. The user name and password are required to enter.
User Name | Enter the login user name for logging in the FTP file server.
Password | Enter the password required for logging in the FTP file server. To change the password, set [Change Password] to and enter the new password in the text box.
Enable SSL | Enables the SSL encryption communication.

### Deleting an FTP server

To delete a selected FTP server, set the checkbox at the left of the FTP server name to and tap [Delete] key.
Back to top