# COPY FUNCTION SETTINGS

## "Initial Status Settings" Tab

Default settings selected with these settings apply to all functions of the machine (not just the copy function).
The copier settings are reset to the initial state when the [POWER] button is turned on, when the [CA] key is tapped, or when the Auto Clear Interval has elapsed. These settings are used to change the default settings for copy mode.

###### List of Set Up Items

Item | Description
--- | ---
Colour Mode | Configure default colour mode settings.
Paper Tray | Specify the paper tray that is selected by default.
Exposure Type | Configure default exposure mode settings.
Copy Ratio | Specify the copy ratio that is selected by default.
2-Sided Copy | Configure the 2-sided mode settings that are selected by default. If this setting is used to change the default setting for the duplex function to any setting other than "1-Side to 1-Side" and the duplex function or automatic document feeder fails or is disabled, the setting will revert to "1-Side to 1-Side".
OUTPUT | Set the print output method and output tray that are selected by default.
Trimming Width Settings | Sets the default trimming width for trimmer function. This option is displayed when the saddle finisher and the trimmer module are installed.
Return to the Defaults | This returns all items to the factory default settings.

## "Copy Function Settings" Tab

The following settings are related to copying.

###### Copy Exposure Adjustment

Adjusts the exposure level when [Auto] is used for the copy exposure.

Item | Description
--- | ---
Colour | Sets the copy exposure level in colour mode for the document glass and for the automatic document feeder.
B/W | Sets the copy exposure level in black & white mode for the document glass and for the automatic document feeder.

###### Rotation Copy Setting

When the original and paper are placed in different orientations, this function automatically rotates the image 90 degrees to enable correct copying on the paper.
Enable the Rotation Copy setting to copy an A5 (5-1/2" × 8-1/2") size original on A5R (5-1/2" × 8-1/2"R) paper.

###### Add or Change Extra Preset Ratios

Add or Change Extra Preset Ratios Add two enlargement preset ratio values (101% to 400%) and two reduction preset ratio values (25% to 99%).
Also, you can change the preset ratio if necessary.
Preset ratios other than added preset ratios cannot be changed.

###### Setting a Maximum Number of Copies

This is used to set the maximum number that can be entered for the number of copies (number of continuous copies). Any number from 1 to 9999 can be specified.

###### Initial Margin Shift Setting

This is used to set the default margin shift amount. Specify a value from 0 mm (0") to 50 mm (2") in increments of 3 mm (1/8") for both the front and reverse sides.

###### Erase Width Adjustment

This is used to set the default erase width for erase function. Specify a value from 0 mm (0") to 25 mm (1") in increments of 3 mm (1/8") for both Edge Clearance Width and Centre Clearance Width.

###### Card Shot Settings

This is used to set the default original size for the card shot function.
Specify a value from 25 mm (1") to 216 mm (8-1/2") in increments of 3 mm (1/8") for both the X (horizontal) and Y (vertical) dimensions of the original.
If the "Fit to Page" checkbox is set to , the [Fit to Page] key always appear on the card shot screen.

###### Automatic Saddle Stitch

Saddle stitch stapling take place automatically when the pamphlet copy function is used.

###### Initial Tab Copy Setting

This is used to set the default image shift width (tab width) for tab copying.
Specify a value from 0 mm (0") to 25 mm (1") in increments of 3 mm (1/8").

###### Disable Registration of Program

This is used to prohibit the deletion and changing of copy settings stored in job programs.

###### Disabling of Bypass-Tray in Duplex Copy

Disables the use of the bypass tray when making 2-sided copies.
The bypass tray is often used to feed label sheets, transparency film, and other special media for which 2-sided copying is prohibited. If a sheet of one of these special media enters the reversing unit, a misfeed or damage to the unit may result. If special media for which 2-sided copying is prohibited is often used, it is recommended that you enable this setting.

###### Disabling of Auto Paper Selection

Disables the Auto Paper Selection function.
When this setting is enabled, automatic selection of paper that is the same size as the original on the document glass or in the automatic document feeder does not take place.

###### Auto Selection Setting of Tray that is Supplied the Paper

When this setting is enabled and paper is loaded into a tray while the machine is on standby in copy mode, that tray is automatically selected.

###### Disabling Registration of Custom Image

Disables storage of a custom image.

###### Disabling sending while copying

Disables the Image Send function during copy.

###### B/W 600 dpi × 600 dpi Scanning Mode for Document Feeder

The resolution for copying in black and white using the automatic document feeder can be changed from 600 × 400 dpi to 600 × 600 dpi (high quality mode).
When high quality mode is used, fine print and thin lines are reproduced with greater clarity, however, the scanning speed is slower.
When high quality mode is not selected, the following conditions must be satisfied in order to scan at 600 × 400 dpi and attain the fastest speed.

- The copy ratio must be set to 100%.
- Do not select a special mode that will change the ratio.
- [Copy of Copy] must not be enabled.
- Do not copy in black and white with the [Colour Start] key.

###### B/W Quick Scan from Document Glass

The resolution for copying in black and white using the document glass can be changed from 600 × 600 dpi to 600 × 400 dpi (high speed mode).
When high speed mode is selected, the first copy time is quicker, however, the copy image is not as clear.
When high quality mode is not selected, the following conditions must be satisfied in order to scan at 600 × 400 dpi and attain the fastest speed.

- The copy ratio must be set to 100%.
- Do not select a special mode that will change the ratio.
- [Copy of Copy] must not be enabled.
- Do not copy in black and white with the [Colour Start] key.

###### Auto Clear Before Copy Job Execution

Enables the Auto Clear function during copy even when a copy job is not completed. This protects the machine from being held due to the incomplete copy job.

## Colour Adjustments

The following settings are related to colour.

### Initial Colour Balance Setting

If you have adjusted the colour balance using the Colour Balance Adjustment of another function and you have registered them in program (up to 48 settings), you can call any of them and set as the standard setting*. If the adjusted setting or the colour balance having the desired colour components is changed, you can use this method to recall the standard setting permanently.
* The default values to be shown when the "Colour Balance" adjustment screen of another function is displayed.

###### Return to the Defaults

The registered adjustment values are returned to the factory defaults (all colours at 8 levels are returned to zero).

### Auto Colour Calibration

Performs automatic colour correction when the colour in colour copies is off. The machine prints a test patch, the test patch is scanned, and the colour is automatically corrected.
After the [Execute] key is tapped and a test patch is printed, a message appears prompting you to begin automatic calibration. Place the test patch on the document glass as shown below (so that the thin line at the edge of the page is to the left).

Lay copy paper (about five sheets) that is the same size as the test patch on top of the placed test patch, gently close the automatic document feeder, and tap the [Execute] key.

- Before executing Auto Colour Calibration, check to see if the registration adjustment is correct. If the registration adjustment is incorrect, perform "Registration Adjustment".
- If the colour is still off after performing Auto Colour Calibration, repeating Auto Colour Calibration once again may improve the colour.

Back to top