# PROTOCOL SETTINGS

## "TCP/IP" Tab

To use the machine on a TCP/IP network, this setting must be enabled.
When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### IPv4 Settings

When using the machine on a TCP/IP (IPv4) network, use this setting to configure the IP address of the machine.

###### DHCP/BOOTP

Use this setting to have the IP address obtained automatically using DHCP (Dynamic Host Configuration Protocol)/BOOTP (Bootstrap Protocol). When this setting is enabled, it is not necessary to manually enter an IP address.
If the machine is used on a TCP/IP network, be sure to enable the "TCP/IP".
If DHCP/BOOTP is used, the IP address assigned to the machine may change automatically. If the IP address changes, printing will not be possible.

###### RARP

Set this option to use the RARP protocol.

###### IPv4 Address

Enter the IP address of the machine.

###### Subnet Mask

Enter the IP subnet mask.

###### Default Gateway

Enter the default gateway address.

### IPv6 Settings

When using the machine on a TCP/IP (IPv6) network, use this setting to configure the IP address of the machine.

###### IPv6

Enable this setting.

###### DHCPv6

Use this setting to have the IP address obtained automatically using DHCP (Dynamic Host Configuration Protocol) v6. When this setting is enabled, it is not necessary to manually enter an IP address.

###### Manual Address/Prefix Length

Enter the IP address and the prefix length (0 to 128) of the machine.

###### Default Gateway

Enter the default gateway address.

- If the machine is used on a TCP/IP network, be sure to enable the "TCP/IP" below.
- In an IPv6 environment, the machine can use LPD or IPP protocol.

- If DHCPv6 is used, the IP address assigned to the machine may change automatically. If the IP address changes, printing will not be possible.

### Ping Command

Checks if the machine can communicate with the PC of the network.
Specify the IP address of the desired PC and tap the [Execute] key. A message indicating a response by the PC or not is displayed.

## "NetWare" Tab

When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### NetWare Settings

###### NetWare

To use the machine on a NetWare network, this setting must be enabled.

###### Frame Type

Select a frame type.
Settings: 802.2, 802.3, SNAP, ETHER-II

###### Operation Mode

Select an operation mode.
Settings: PSERVER, RPRINTER

###### Printer Name

Enter the printer name.

### PSERVER Settings

###### Print Server Name

Enter a print server name.

###### Login Password

Enter the login password.
To change the password, set [Change Password] to .

###### Check Interval

Enter a job check interval.

###### Bindery Mode

Set this option to use the Bindery mode.

###### File Server Name 1 to 8

Enter a file server name.

###### NDS Tree

Enter the NDS tree name.

###### NDS Context

Enter the NDS context.

### RPRINTER Settings

###### Print Server Name 1 to 8

Enter a print server name.

###### Job Timeout

Enters a job timeout.

## "EtherTalk" Tab

When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### EtherTalk Settings

###### EtherTalk

To use the machine on an EtherTalk network, this setting must be enabled.

###### Zone Name

Enter a zone name.

###### Printer Name

Enter the printer name.

## "NetBIOS" Tab

When settings are changed, the changes will take effect after the machine is restarted. To restart the machine, see "TURNING ON OR OFF THE POWER AND RESTARTING THE MACHINE".

### NetBIOS Settings

###### NBT/WINS

To use the machine on a NetBIOS network, this setting must be enabled.
Back to top