# USING MANUAL FINISHING

## Overview

Change from the Home Screen or each mode to manual finishing mode, and carry out the following procedure.

- SELECTING MANUAL FINISHING MODE

## Operation

1. #### Set the guides to the size of the paper

   Grasp the guide lock lever to adjust the guide.
   When you have finished the adjustment, release the lock lever.

   When loading paper larger than A4R, or 8-1/2" × 11"R, extend the bypass tray all the way out. If it is not pulled all the way out, the size of the loaded paper will not be detected correctly.

2. #### Load paper into the upper or lower tray

   The paper orientation varies depending on the manual finishing function.

   - CHANGING TYPE AND SIZE OF PAPER
   - ORIENTATION
   - Up to 200 sheets of paper can be loaded into each of the upper and lower trays.
   - Insert the paper along the guides all the way into the tray.
   - If the guide width is not correctly adjusted to match the paper width, paper may be jammed, skewed, or crease. Adjust the paper guides to fit the width of the paper.

3. #### Select the appropriate finishing method

   - STAPLE FUNCTION
   - PAPER FOLDING FUNCTION
   - PUNCH FUNCTION

4. #### Change the paper tray or output tray as required

   - TO CHANGE THE PAPER TRAY
   - TO CHANGE THE OUTPUT TRAY

5. #### Tap the [Start] key to begin manual finishing

   ###### To stop manual finishing:

   Tap the [Stop] key.

Back to top