# FINISHER

## Overview

This device outputs sorted paper while staggering each set of paper. As needed, it staples each set.
To punch holes in printed paper, install an optional hole punch module.

- Function names
- Supplies
- Finisher maintenance

Function names
The following describes the parts that appear when the finisher is open.
×
Output tray
Stapled and offset output is delivered to this tray.
The tray is slidable. Extend the tray for printing on large-size paper (A3W, A3, A4R, B4, B5R, 8K, 16KR, 12" x 18", 11" x 17", 8-1/2" x 14", 8-1/2" x 13", 8-1/2" x 13-1/2", 8-1/2" x 13-2/5", 8-1/2" x 11"R and 7-1/4" x 10-1/2"R sizes).
×
Lever
Use this lever to move the finisher in order to remove a paper misfeed, replace staples, or remove a staple jam.
×
Punch waste box (when a punch module is installed)
This stores punch waste discharged from punching.
×
Front cover
Open this cover to remove a paper misfeed, replace staples, remove a staple jam, or remove the punch scrap case.
×
Staple case
This holds the staple cartridge. Pull the case out to replace the staple cartridge or remove a staple jam.
×
Staple case release lever
Use this lever to remove the staple case.
Tap the name to make its details pop up.

- A finisher cannot be installed simultaneously with a saddle finisher.
- Exercise caution when you turn on the power and when printing is taking place, as the output tray may move up and down.

Supplies
The finisher requires the following staple cartridge:
Staple cartridge (approx. 5000 staples per cartridge x three cartridges)
MX-SCX1
Finisher maintenance
When the staple cartridge runs out of staples, a message will appear in the operation panel. Follow the operation procedure to replace the staple cartridge.

## Operation

Replacing the cartridge
Open the cover.
While pressing the lever over to the left, slide the finisher to the left until it stops.
Gently slide the finisher until it stops.
Lower the staple case release lever and remove the staple case.
Pull the staple case out to the right.
Remove the empty staple cartridge from the staple case.
Insert a new staple cartridge into the staple case as shown.
Push the staple cartridge in until it clicks into place.
Replace the staple case.
Push the staple case in until it clicks into place.
Slide the finisher back to the right.
Gently slide the finisher back to the right until it locks into its original position.
Close the cover.
Make a proof copy in staple sort function to verify that stapling takes place correctly.
Make a proof copy in staple sort function to verify that stapling takes place correctly.
Back to top