# ADJUSTING THE SHARPNESS OF AN IMAGE(SHARPNESS)

## Overview

This function adjusts the sharpness to make a sharper or softer image.
Sharpness must be specified before scanning the original.

## Operation

Tap the [Others] key, and tap the [Sharpness] key.
Tap or slide the slider to adjust the sharpness.
After the settings are completed, tap and [Back] keys in sequence.
To cancel the sharpness setting:
Tap the [Off] key.
Place the original and tap the [Preview] key.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

To cancel all settings:
Tap the [CA] key.
Tap the [Start] key to start copying.
When making only one set of copies, you do not need to specify the number of copies.
To make two or more sets of copies:
Tap the copies display key to specify the number of copies.
Back to top