# ADJUSTING RESOLUTION WHEN SCANNING(RESOLUTION)

This function adjusts the resolution when scanning the original, enabling the high-quality output or speed-priority output according to the application.

Resolution must be specified before scanning the original.

Touch the [Others] key, and tap the [Scan Resolution] key.
Select the resolution.
The resolution can be set to both the document feeder and document glass.
After the settings are completed, tap and [Back] keys in sequence.
Place the original and tap the [Preview] key.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Tap the [Start] key to start copying.
When making only one set of copies, you do not need to specify the number of copies.
To make two or more sets of copies:
Tap the copies display key to specify the number of copies.
Back to top