# POLLING RECEPTION USING F-CODES

## Overview

This function enables your machine to call another machine and initiate reception of a fax stored in an F-code memory box (polling memory) in the other machine. During the polling operation, your machine must correctly specify the F-code (sub-address and passcode) configured in the other machine. Otherwise, polling reception will not take place.

- Verify the F-code (sub-address and passcode) of the memory box in the other machine before you perform F-code polling reception.
- The receiving machine bears the telephone charges of the transmission.
- If necessary, use the F-code polling reception in combination with a broadcast transmission or timer transmission. Only one polling reception with a timer setting can be stored at a time.

- SPECIFYING THE TIME FOR COMMUNICATION(TIMER)

- Polling multiple machines (serial polling) is not possible.
- Make sure there is no original in the machine when using the F-code for the polling reception function.
- The polling reception using the F-code cannot be registered as a "favourite" item.

## Operation

Tap the [Others] key, and tap the [Polling] key.
A checkmark appears on the icon.
After the settings are completed, tap the [Back] key.
To cancel the Polling setting:
Tap the [Polling] key to clear the checkmark.
Specify the destination.

1. (1) Enter the destination line number using the numeric keys.
2. (2) Tap the [Sub Address] key.
   Symbol "/" is entered.
3. (3) Enter the sub-address using the numeric keys.
4. (4) Tap the [Passcode] key.
   Symbol "/" is entered.
5. (5) Enter the passcode using the numeric keys.

- If the sub-address and passcode are already registered, you can select a one-touch key as well.
- If the passcode is omitted for the memory box of destination machine, you can skip Steps (4) and (5).
Tap the [Start] key.
Your machine will call the other machine and initiate reception of the fax.
Back to top