# TRANSMISSION USING THE SPEAKER

## Overview

When the speaker is used to dial, the fax is sent after the number is dialled and the connection is established.

- If a person answers, you will be able to hear his or her voice, but you will not be able to speak.
- When the speaker is used, transmission takes place without scanning the original into memory.
- A destination that includes an F-code (sub-address and passcode) cannot be used.
- A one-touch key that has multiple destinations or has a non-fax destination cannot be used.
- In speaker mode, the [Preview] key cannot be used for transmission.

## Operation

Place the original.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Tap the [Speaker] key.
When the connection is established, you will hear the dial tone through the machine's speaker.
After tapping the [Speaker] key, use the slider that is displayed when you tap the [Speaker Volume] key or use key to adjust the volume of the speaker.
Specify the destination fax number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

A one-touch key in which multiple destinations are stored cannot be used.
When the connection is made, tap the [Start] key to begin transmission.
To cancel transmission:
To stop transmission, tap the [Stop] key. To stop communication, tap the [Speaker] key.
Back to top