# SELECTING NETWORK SCANNER MODE

You can select the network scanner mode from the Home Screen or from each operation mode as follows:

## Operation

### Changing modes from the Home Screen

1. #### Tap the icon indicating the network scanner mode

   Tap one of [E-mail], [FTP/Desktop], [Network Folder], and [Internet Fax].
   The initial screen of the selected mode is displayed.

### Changing mode from each mode

1. #### Tap on the mode display

2. #### Tap [Image Send]

   By default, the screen changes to the fax mode screen.

   ###### To change the screen that is initially displayed when the [Image Send] in the mode display is tapped:

   In "Setting mode (administrator)", select [System Settings] → [Image Send Settings] → [Operation Settings] → [Default Settings] → [Default Display Setting].

3. #### Tap and then tap one of [E-mail], [FTP/Desktop], [Network Folder], and [Internet Fax]

   The initial screen of the selected mode is displayed.
   In "Setting mode", by selecting [System Settings] → [Image Send Settings] → [Fax Settings] → [Default Settings] → [Address Book Default Selection] and setting the [Higher priority is given to the display of address book.] checkbox to , the Address Book in the selected mode is displayed.

Back to top