# RESENDING TO UNSUCCESSFUL BROADCAST TRANSMISSION DESTINATIONS

## Overview

The results of a completed broadcast transmission can be checked in the job status screen. If transmission to any of the destinations failed, resend the image to those destinations.

## Operation

Tap the job status display.
After tapping the appropriate mode tab, tap the [Complete] key.
If the broadcast transmission included destinations of different modes, the same broadcast transmission key will appear in each of those modes.
After tapping the key of the completed broadcast transmission, tap the [Check Details of Selected Job] key on the action panel.
"Broadcast xxxx" will appear as the destination of the broadcast job key. The job control number that appeared on the touch panel when scanning ended appears in "xxxx".
After tapping the [Sending Failed] tab, tap the [Resending to all unsuccessful transmission destinations] key on the action panel to resend the image.
The steps to follow after the [Resending to all unsuccessful transmission destinations] key is tapped differ depending on whether or not document filing is used.

- Using document filing:
  You will return to the document filing resend screen with the unsuccessful destinations entered.
  Perform the document filing resend procedure. (There is no need to re-scan the original.)
- Not using document filing:
  You will return to the base screen with the unsuccessful destinations entered. Place the original and perform the steps of the broadcast transmission.

Back to top