# RECEIVING INTERNET FAXES AUTOMATICALLY

## Overview

The Internet fax function periodically connects to the mail server (POP3 server) and checks whether or not Internet faxes have been received. When faxes have been received, the faxes are automatically retrieved and printed.
In the default setting, this function checks for reception once every five minutes.

- If faxes will be received at night, keep the main power switch of the machine in the "" position.
- If the machine is out of paper or there is no paper that matches the size of the received fax, a message will appear in the touch panel. Follow the instructions in the message to load an appropriate size of paper.
- You can print the received Internet fax data at the specified time.
  - PRINTING RECEIVED DATA AT A SPECIFIED TIME
- You can print the received Internet fax data when a password has been entered.
  - PRINTING A PASSWORD-PROTECTED FAX(HOLD SETTING FOR RECEIVED DATA PRINT)
- You can print, forward, or save the received Internet fax data after checking it.
  - CHECKING THE IMAGE BEFORE PRINTING
  - FORWARDING RECEIVED DATA MANUALLY
  - SAVING RECEIVED DATA

## Operation

The machine rings and fax reception begins automatically.
A beep sounds when reception ends.
The fax is automatically printed.
Back to top