# SCANNING AN ORIGINAL AS TWO SEPARATE PAGES(DUAL PAGE SCAN)

## Overview

The left and right sides of an original are scanned as two separate pages. This function is useful when you wish to successively scan each page of a book or other bound document.
When using dual page scan, the original must be placed on the document glass.

Original scan size | Transmitted image
--- | ---
A3 (11" x 17") x 1 page | A4 (8-1/2" x 11") x 2 pages

- This function is available when the original size setting is set to [Auto].
- Note that "Centre Erase" and "Edge + Centre Erase" cannot be used.

## Operation

Place the original on the document glass.

- DOCUMENT GLASS

Align the centre of the original with the appropriate size mark .
Specify the destination.

- RETRIEVING A DESTINATION FROM AN ADDRESS BOOK
- VIEWING A LIST OF THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- ENTERING AN ADDRESS MANUALLY
- SPECIFYING A NETWORK FOLDER
- RETRIEVING A DESTINATION FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND

Tap the [Others] key, and tap the [Dual Page Scan] key.
A checkmark appears on the icon.
After the settings are completed, tap the [Back] key.
To cancel the Dual Page Scan setting:
Tap the [Dual Page Scan] key to clear the checkmark.
Tap the [Start] key to start scanning of the original.
Tap the [Preview] key to check the preview of an image before sending a fax. For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED". However, settings for this function cannot be changed in the preview screen.
When scanning finishes, place the next original and tap the [Start] key.
Repeat until all pages have been scanned and then tap the [Read-End] key.
A beep will sound to indicate that transmission has ended.
Back to top