# SECURITY SETTINGS

The following is a list of setting mode items, factory default settings and restrictions for each item.
Depending on the machine specifications and peripheral devices installed, it may not be possible to use some settings.
U: General user; A: System administrator/Administrator

Item | Factory default setting | U | A
--- | --- | --- | ---
| Security Settings
| Other Settings
| No | Yes
| Restrict Print Jobs other than the current Print Hold Job
| Enabled | No | Yes
| Restrict Operation
| Force Retention | No | Yes
| Change Password
| - | No | Yes
| Port Control
| No | Yes
| Server Port
| No | Yes
| HTTP
| Enabled | No | Yes
| Port Number
| 80 | No | Yes
| HTTPS
| Enabled | No | Yes
| Port Number
| 443 | No | Yes
| FTP Print
| Enabled | No | Yes
| Port Number
| 21 | No | Yes
| Raw Print
| Enabled | No | Yes
| Port Number
| 9100 | No | Yes
| LPD
| Enabled | No | Yes
| Port Number
| 515 | No | Yes
| IPP
| Enabled | No | Yes
| Port Number
| 631 | No | Yes
| IPP-SSL
| Disabled | No | Yes
| Port Number
| 443 | No | Yes
| Tandem Output Receive
| Enabled | No | Yes
| Port Number
| 50001 | No | Yes
| PC Scan
| Enable | No | Yes
| Port Number
| 52000 | No | Yes
| Remote Operation Panel
| Enabled | No | Yes
| Port Number
| 5900 | No | Yes
| SNMPD
| Enabled | No | Yes
| Port Number
| 161 | No | Yes
| Telnet
| Enabled | No | Yes
| NBT/WINS
| Disabled | No | Yes
| JCP
| Disabled | No | Yes
| RARP
| Disabled | No | Yes
| SMTP
| Enabled | No | Yes
| WSD
| Enabled | No | Yes
| USB-Device Expansion*1
| Enabled | No | Yes
| Sharp OSA (Expansion Platform)
| No | Yes
| HTTP
| Enabled | No | Yes
| Port Number
| 10080 | No | Yes
| HTTPS
| Enabled | No | Yes
| Port Number
| 10443 | No | Yes
| Client Port
| No | Yes
| HTTP
| Enabled | No | Yes
| HTTPS
| Enabled | No | Yes
| FTP
| Enabled | No | Yes
| FTPS
| Enabled | No | Yes
| SMTP
| Enabled | No | Yes
| SMTP-SSL
| Enabled | No | Yes
| POP3
| Enabled | No | Yes
| POP3-SSL
| Enabled | No | Yes
| SNMP-TRAP
| Enabled | No | Yes
| Port Number
| 162 | No | Yes
| Notify Job End
| Enabled | No | Yes
| LDAP
| Enabled | No | Yes
| LDAP-SSL
| Enabled | No | Yes
| SMB/WINS
| Enabled | No | Yes
| SNTP
| Disabled | No | Yes
| mDNS
| Enabled | No | Yes
| Tandem Output Send
| Enabled | No | Yes
| Data Backup (Send)
| Enable*5 | No | Yes
| Filter Setting
| Disabled | No | Yes
| IP Address Filter Settings
| No | Yes
| Filter Mode
| Allowed | No | Yes
| Filter Addresses 1 to 4
| No | Yes
| Start IP Address
| 0.0.0.0 | No | Yes
| End IP Address
| 0.0.0.0 | No | Yes
| MAC Address Filter Settings
| No | Yes
| Filter Addresses 1 to 10
| 000000000000 | No | Yes
| SSL Settings
| No | Yes
| Server Port
| No | Yes
| HTTPS
| Enabled | No | Yes
| IPP-SSL
| Disabled | No | Yes
| Redirect HTTP to HTTPS in Device Web Page Access
| Disabled | No | Yes
| Client Port
| No | Yes
| HTTPS
| Enabled | No | Yes
| FTPS
| Enabled | No | Yes
| SMTP-SSL
| Enabled | No | Yes
| POP3-SSL
| Enabled | No | Yes
| LDAP-SSL
| Enabled | No | Yes
| Level of Encryption
| Low | No | Yes
| Certificate Information
| - | No | Yes
| IEEE802.1X Setting
| No | Yes
| IEEE802.1X Authentication
| Disabled | No | Yes
| EAP Authentication Method
| EAP-TLS | No | Yes
| EAP User Name
| - | No | Yes
| Password
| - | No | Yes
| Server Authentication
| Enabled | No | Yes
| EAP Timeout
| 10 seconds | No | Yes
| Number of EAP Retries
| 3 times | No | Yes
| Certificate Information
| - | No | Yes
| Data Clearance Settings*2
| Disable | No | Yes
| Release Lock on File/Folder Operation*2
| - | No | Yes
| IPsec Settings
|  | No
| IPsec Settings
| Disabled | No | Yes
| IKEv1 Settings
|  | No
| Pre-Shared Key
| - | No | Yes
| SA Lifetime (time)
| 28800 seconds | No | Yes
| SA Lifetime (size)
| 28800 KB (10 mm (1/2")) | No | Yes
| IKE Lifetime
| 30 seconds | No | Yes
| IPsec Rules
| - | No | Yes
| Hidden Pattern Print
| No | Yes
| Default Settings
| Hidden Pattern Print Setting
| Standard | No | Yes
| Exposure
| Standard | No | Yes
| Font Size
| 48 points | No | Yes
| Angle
| 0 deg. | No | Yes
| Font Style
| Standard | No | Yes
| Camouflage Pattern
| Pattern 1 | No | Yes
| Print Method
| Character stand out. | No | Yes
| Print Contents Setting
| No | Yes
| Pre-Set Word
| Enabled, DO NOT COPY | No | Yes
| Pre-set Text
| ON | No | Yes
| Unit Serial Number
| Disabled | No | Yes
| Account Job ID
| Disabled | No | Yes
| Login Name/User Number
| Disabled | No | Yes
| Control No.
| Disabled | No | Yes
| Date/Time
| Disabled | No | Yes
| Disable Direct Entry
| Disabled | No | Yes
| Contrast
| No | Yes
| Black
| 5 | No | Yes
| Custom Text Registration
| - | No | Yes
| Tracking Information Print
| - | No | Yes
| Tracking Information Print Setting
| Disabled | No | Yes
| Print Information
| No | Yes
| Unit Serial Number
| Enabled | No | Yes
| Text
| Disabled | No | Yes
| Account Job ID
| Enabled | No | Yes
| Login Name/User Number
| Enabled | No | Yes
| Date/Time
| Enabled | No | Yes
| Print Position
| No | Yes
| Vertical Position
| No | Yes
| Print Upper Side of Paper
| Disabled | No | Yes
| Print Lower Side of Paper
| Enabled | No | Yes
| Horizontal Position
| No | Yes
| Print Left Side of Paper
| Enabled | No | Yes
| Print Right Side of Paper
| Disabled | No | Yes
| Select the Job to Print
| No | Yes
| Copy
| Enabled | No | Yes
| Printer
| Enabled | No | Yes
| Prints (Document Filing)
| Enabled | No | Yes
| Internet Fax Receive*3
| Enabled | No | Yes
| Fax Receive*4
| Enabled | No | Yes
| List Prints
| Enabled | No | Yes
| Initialize Private Data/Data in Machine
| - | No | Yes

*1 Displayed when the application communication module or external account module product key is enabled.
*2 Displayed when the data security kit is enabled
*3 Displayed when the Internet fax function is enabled.
*4 Displayed when the fax function is enabled.

*5 Disabled when the data security kit is installed

Back to top