# AUTOMATIC REDUCTION OF THE TRANSMITTED IMAGE

If the width of the transmitted image is larger than the width of the paper in the receiving machine, the image will be automatically reduced to fit the receiving machine's paper width.
Example: Reduced sizes and reduction ratios

Transmitted image width | Receiving machine's paper width | Reduced size | Ratio
--- | --- | --- | ---
A3 (11" x 17") | B4 | B4 | 1:0.84
A3 (11" x 17") | A4 (8-1/2" x 14", 8-1/2" x 11") | A4R (8-1/2" x 14", 8-1/2" x 11"R) | 1:0.71
B4 | A4 (8-1/2" x 11") | A4R | 1:0.84

To cancel the Auto Reduction Sending setting:
In "Setting mode", select [System Settings] → [Image Send Settings] → [Fax Settings] → [Send Settings] → [Auto Reduction Sending Setting].
If this setting is disabled, the image will be sent at full size and part of the image may be cut off.
Back to top