# FORWARDING RECEIVED FAXES(FAX DATA FORWARD)

## Overview

When the machine cannot print because it is out of paper or out of toner, received faxes can be forwarded to another previously stored fax machine.

This function is convenient in an office or work area that has two or more telephone lines and another fax machine is connected to a different line than the machine.

- If some pages of a fax that is being forwarded were successfully printed, only those pages that were not printed will be forwarded.
- A forwarded fax becomes a fax transmission job. If transmission does not take place because the transmission was cancelled or an error occurred, the fax will be held in memory until it can be printed.
- All faxes received are forwarded. Note, however, that faxes received and stored in an F-code confidential memory box cannot be forwarded.

## Operation

Tap the [Settings] key on the Home screen.
Select [System Settings] and tap the [Fax Data Receive/Forward] key.
Tap the [Fax Settings] key.
Tap the [Execute] key in [Forward Received Data] to begin forwarding.
If a password entry screen appears, the "Hold Setting for Received Data Print" has been enabled. Enter the password using the numeric keys to begin forwarding.

- PRINTING A PASSWORD-PROTECTED FAX (HOLD SETTING FOR RECEIVED DATA PRINT)

Back to top