# IMAGE SEND SEQUENCE

First, to place the machine in a desired image send mode, tap the appropriate icon in the Home screen.

- SELECTING NETWORK SCANNER MODE

Place the original.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Enter the destination.
Tap the address key to directly enter the destination, and specify the address to send scan data.

- RETRIEVING A DESTINATION FROM AN ADDRESS BOOK
- VIEWING A LIST OF THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- ENTERING AN ADDRESS MANUALLY
- SPECIFYING A NETWORK FOLDER
- RETRIEVING A DESTINATION FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND

Configure the scan settings.
Specify the original scan size, exposure, file format, and other items.
If necessary, you can refer to the following functions for the setting.

- SCANNING AND SENDING ORIGINALS COLLECTIVELY
- ADJUSTING COLOURS AND SHADING
- SCANNING ORIGINALS

- AUTOMATICALLY SCANNING BOTH SIDES OF AN ORIGINAL(2-SIDED ORIGINAL)
- SCAN SIZE AND SEND SIZE(ENLARGE/REDUCE)
- SPECIFYING THE ORIGINAL SCAN SIZE IN PAPER SIZE
- SPECIFYING THE ORIGINAL SCAN SIZE USING NUMERIC VALUES
- SPECIFYING THE SEND SIZE OF THE IMAGE
- CHANGING THE EXPOSURE AND ORIGINAL IMAGE TYPE
- CHANGING THE RESOLUTION
- CHANGING FORMAT IN SCAN OR DATA ENTRY MODE
- CHANGING FORMAT IN INTERNET FAX MODE
- CHANGING COLOUR MODE

Set Others.
Use Others other than the time when using scan settings such as sending two pages as a single page or sending originals of different sizes at the same time.
Send the original.
Tap the [Start] key.
You can check the preview of an image by tapping the [Preview] key.
When the original is placed on the document glass:
Repeat the placing original and transmission procedures until all originals have been sent. After scanning all originals, tap the [Read-End] key.
Back to top