# RECEIVING A FAX MANUALLY

## Overview

A fax can be received manually using the touch panel (manually).

- When answering the telephone by tapping the [Speaker] key, you will be able to hear the voice of the caller, but you will not be able to speak.
- You can receive a fax after answering a call on an extension telephone. Remote reception can also be used to receive a fax.
  - RECEIVING A FAX AFTER ANSWERING A CALL ON THE EXTENSION TELEPHONE (REMOTE RECEPTION)

###### To switch between auto reception and manual reception modes:

In "Setting mode", select [System Settings] → [Receive/Forward Settings] → [Fax Settings] → [Receive Settings].

## Operation

Tap the [Speaker] key or pick up the receiver of extension telephone while the telephone is ringing.
When the [Speaker] key is tapped, the [Manual Reception] and appear.

- Adjust the volume by using the slider that is displayed when you tap the [Speaker Volume] key or using .
- If the received fax data remains unprinted, it will cause the fax memory to fill up, which may prevent some faxes from being received. If this function is enabled, you should print the received data as soon as possible without leaving it in the fax memory.
  You can view the remaining fax memory capacity on the fax mode base screen.

Tap the [Manual Reception] key to receive a fax.
Back to top