# CLEANING THE MAIN CHARGER OF THE PHOTOCONDUCTIVE DRUM

## Overview

If black lines lines appear even after you have cleaned the document glass and automatic document feeder, use the charger cleaner to clean the main charger that charges the photoconductive drum.

- If cleaning the main charger of the photoconductive drum does not solve the problem, pull the knob out and push it back three more times.
- When pulling and pushing the knob to clean the charger, pull and push the knob slowly from one end to the other.

## Operation

Open the front cover.
Release the toner collection container.
Press up the toner collection container release lever.
The toner collection container will fall forward as shown.
Gently support the container with your hands as you let it fall forward as far as it will go.
Clean the main charger.
Gently pull the charger cleaner all the way up, and gently push it in.
Push the toner collection container into the machine.
Push the container in until it clicks into place.
Close the front cover.
Back to top