# SENDING TWO PAGES AS A SINGLE PAGE(Multi Shot)

## Overview

Reduce two original pages to the equal size and sent them as a single page. This function is convenient when you have a large number of original pages and wish to reduce the number of pages sent.
For the standard size (A4 (8-1/2" x 11") or B5 or A5 (5-1/2" x 8-1/2")), original pages are scanned from both the single pass feeder and document glass.

- Transmission is not possible at a size smaller than the original size.
- The 2in1 is only available for originals with A4 (8-1/2" x 11") or B5 or A5 (5-1/2" x 8-1/2") size.
- This function cannot be used in direct transmission mode or when the speaker is used to dial.
- When the scan size of the original is specified by numeric values, this function cannot be used.
- This function cannot be used together with Dual Page Scan or Card Shot.

## Operation

Place the original.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Enter the destination fax number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

Tap the [Others] key, and tap the [Multi Shot] key.
A checkmark appears on the icon.
After the settings are completed, tap the [Back] key.
To cancel the Multi Shot setting:
Tap the [Multi Shot] key to clear the checkmark.
Tap the [Original] key.
Tap the [Image Orientation] key with the same orientation as the placed original.
If this setting is not correct, a suitable image may not be transmitted.
After the settings are completed, tap .
Tap the [Start] key to start scanning of the original.

- If you inserted the original pages in the document feeder tray, all pages are scanned.
  A beep will sound to indicate that scanning and transmission have ended.
- If you placed the original on the document glass, scan each page one at a time.
  When scanning finishes, place the next original and tap the [Start] key. Repeat the procedure until all pages have been scanned and then tap the [Read-End] key.
  A beep will sound to indicate that scanning and transmission have ended.

- Tap the [Preview] key to preview the output image before sending it. After you have scanned an original by tapping the [Preview] key, tap the [Additional Scan] key to scan the next original. Tap the [Start] key to start sending an image.
  For more information, see "CHECKING THE IMAGE TO BE TRANSMITTED".
- If you tap the [Function Rev.] key on the scan confirmation screen, you can change the exposure, resolution, scan size, and send size.
  (However, when scanning each even-numbered page of the original, only the exposure can be changed.)
Back to top