# WHEN A COMMUNICATION ERROR OCCURS

If a communication error occurs or the other fax machine does not answer the call within a preset period of time, transmission will automatically be attempted again after a preset interval This function only operates in memory transmission mode.
In direct transmission mode, transmission will not automatically be attempted again
To cancel the transmission:
Cancel it from the job status screen.

- STOPPING/DELETING A JOB IN PROGRESS OR RESERVED

To set the number of recall attempts and the interval between attempts when a transmission fails due to an error:
In "Setting mode", select [System Settings] → [Image Send Settings] → [Fax Settings] → [Send Settings] → [Recall in Case of Communication Error].
The factory default setting is one attempt at 3-minute intervals.
Back to top