# ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS

Tap numeric keys to enter the destination fax number.
If you want to cancel the PBX settings* temporarily when sending a fax:
Tap the [R] key before entering a fax number.
* This function is not available in some countries and regions.

If you want to enter a pause between digits of the number:
The [Pause] key appears on the numeric keys when the destination fax number is entered.
Tap the [Pause] key to enter a hyphen (-).
If you want to specify multiple addresses, tap and enter the number of the next address.

You can also tap [Pause] key to specify multiple destinations.

If an incorrect number is entered:
Tap the [C] key to clear the number and enter the correct number.

## ENTERING A PAUSE BETWEEN DIGITS OF THE NUMBER

Enter a pause after the number used to dial out from a PBX (for example, after "0"), or after the country code when dialling an international number.
Tap the [Pause] key.
A hyphen "-" is entered when the [Pause] key is tapped once.
The [Pause] key appears on the numeric keys when the destination fax number is entered.
If an incorrect number is entered:
Tap the [C] key to clear the number and enter the correct number.
Back to top