# INITIATING POLLING RECEPTION MANUALLY

## Overview

Use the manual polling reception when you must start polling after listening to a recorded greeting, such as when using a fax information service.

- Make sure there is no original in the machine when using the polling reception function.
- This function cannot be used to poll multiple machines (serial polling).
- The function can only be used when the other machine is Super G3 or G3 compatible and has a polling function.

The receiving machine bears the expense (phone charges) of the polling reception.

## Operation

Tap the [Speaker] key.
You will hear the dial tone through the machine's speaker.
Enter the destination fax number.

- ENTERING A DESTINATION NUMBER USING THE NUMERIC KEYS
- RETRIEVING A DESTINATION NUMBER FROM AN ADDRESS BOOK
- THE SELECTED DESTINATIONS
- USING A SEARCH NUMBER TO RETRIEVE A DESTINATION
- RETRIEVING A DESTINATION NUMBER FROM A GLOBAL ADDRESS BOOK
- USING A TRANSMISSION LOG TO RESEND
- SENDING BY CHAIN DIALLING

One-touch key for a contact or group in which multiple destinations are stored, and one-touch key for which an address other than fax number is stored cannot be used.
After tapping the [Speaker] key, you can tap the [Speaker Volume] key to adjust the volume of the speaker.
Tap the [Others] key, and tap the [Polling] key to receive originals (data).
A checkmark appears on the icon.
To cancel the Polling setting:
Tap the [Polling] key to clear the checkmark.
Back to top