# CHANGING FORMAT IN INTERNET FAX MODE

## Overview

Change the file format (file type and compression mode) for sending a scanned image in Internet Fax mode.
The file format for sending an Internet fax is normally set to [TIFF-F]. If the destination Internet fax machine does not support full mode (it only supports simple mode), select [TIFF-S].
When [TIFF-S] is selected, the transmission settings are restricted as follows:

- Resolution: The selections are [200x100dpi] and [200x200dpi].
  If [TIFF-S] is selected after [200x400dpi], [400x400dpi] or [600x600dpi] is selected, the resolution automatically changes to [200x200dpi].
- Send size: Always A4R (8-1/2" x 11"R).
  If [TIFF-S] is selected after the send size is changed, the send size is automatically fixed to A4R (8-1/2" x 11"R). If a size larger than A4 (8-1/2" x 11") is scanned, the size will automatically be reduced to A4R (8-1/2" x 11"R). When this format is included in a broadcast transmission, the image will be transmitted to all destinations in A4R (8-1/2" x 11"R).
- Others: When a ratio setting is selected and the original size is entered, Dual Page Scan, Card Shot, 2in1, 4in1, or Mixed Size Original cannot be used.

## Operation

Tap the [File Format] key.
Tap the [TIFF-S] or [TIFF-F] key to specify the file format.
If you selected [TIFF-F], select the compression mode.
After the settings are completed, tap .
Back to top