# SPECIFYING A PAPER POSITION(POSITION IMAGE)

## Overview

This function moves the scanned original to a specified position to make a copy.
You can make a copy in any desired position as you can fine adjust the position.
Position Image must be specified before scanning the original.

## Operation

Tap the [Others] key, and tap the [Position Image] key.
Sets a movement distance.

- Tap the area indicating the movement distance on the front or reverse side, and enter the distance using numeric keys.
- To quickly set the area, first specify a value close to the desired value by the numeric keys, then adjust it with .
- If you set the [Adjust 2nd pg value to 1st.] checkbox to , goes out and you can set sides 1 and 2 separately.

After the settings are completed, tap and [Back] keys in sequence.
To cancel the Position Image setting:
Tap the [Clear] key.
Place the original and tap the [Preview] key.
Place the original in the document feeder tray of the automatic document feeder, or on the document glass.

- AUTOMATIC DOCUMENT FEEDER
- DOCUMENT GLASS

Check the preview image in the preview screen.
Check whether or not settings produce the required results.
To cancel all settings:
Tap the [CA] key.
Tap the [Start] key to start copying.
When making only one set of copies, you do not need to specify the number of copies.
To make two or more sets of copies:
Tap the copies display key to specify the number of copies.
Back to top