# PUNCH MODULE

## Overview

This device can be installed on a finisher or saddle finisher to punch holes in paper to be output.
Discarding punch waste
Punch waste from punched holes is collected in the punch waste box.
Follow the operation procedure to replace punch waste.

## Operation

- Finisher installed
- Finisher (large stacker) installed
- Saddle finisher installed
- Saddle finisher (large stacker) installed

Finisher installed
Open the cover.
While pressing the lever over to the left, slide the finisher to the left until it stops.
Gently slide the finisher until it stops.
Grasp the punch waste box handle, gently pull out the box, and discard the punch waste.
Discard the punch waste in a plastic bag or other container, taking care not to let the waste scatter.
Gently push the box back in.
While pressing the lever over to the left, slide the finisher to the left until it stops.
Gently slide the finisher until it stops.
Close the cover.
Finisher (large stacker) installed
Open the front cover of the punch module.
Pull out the punch waste box and discard the punch waste.
Discard the punch waste in a plastic bag or other container, taking care not to let the waste scatter.
Replace the punch waste box.
If the punch waste box is not replaced properly, printing will not be possible using the punch function.
Close the cover of the punch module.
Saddle finisher installed
Open the front cover.
Pull out the punch waste box and discard the punch waste.
Discard the punch waste in a plastic bag or other container, taking care not to let the waste scatter.
Replace the punch waste box.
Close the front cover.
Saddle finisher (large stacker) installed
Open the front cover of the punch module.
Pull out the punch waste box and discard the punch waste.
Discard the punch waste in a plastic bag or other container, taking care not to let the waste scatter.
Replace the punch waste box.
If the punch waste box is not replaced properly, printing will not be possible using the punch function.
Close the cover of the punch module.
Back to top