# FILE TRANSMISSION

## Overview

The settings used when the file was stored with document filing are stored, and thus the file can be transmitted using those settings. If needed, you can also change the transmission settings to modify the retrieved file.

A stored print job cannot be transmitted. (However, if the job has been filed by specifying retention in the printer driver, it can be transmitted as long as RGB is selected for "RIP format" in the [Printer Features] button setting in the [Advanced] tab.)

- These transmission methods require installation of the corresponding options.
- If any of the following other modes were included in the saved file, the file cannot be transmitted.
  "Pamphlet Copy", "Covers/Inserts", "Photo Repeat", "Multi-Page Enlargement", " 2in1" for copying.
- If any of the following other modes were included in the saved file, the file can be transmitted, but other functions cannot be executed.
  "Margin Shift", "Transparency Inserts", "Book Copy", "Tab Copy", "Stamp", all "Colour Adjust" menu items, "Centring"
- Depending on the reduction or enlargement ratio used when storing a file, it may not be possible to send the stored file using a selected resolution setting. In this event, try changing the resolution.
  However, when sending a stored file by Internet fax, transmission may not be possible even if the resolution is changed.

## Operation

After selecting the desired file, follow the steps below.

- SELECTING A FILE TO RETRIEVE

Tap the [Send] key on the action panel.
Select settings for sending.
Tap the [Start] key.
Back to top